SEISHAZARD v1.0 TRIAL — QUICK START

1. Launch SeisHazard.exe.
2. Review the Site and bundled seismic-source inputs in Input Manager.
3. Select one or more built-in GMPEs.
4. Review Analysis settings and return periods.
5. Use Validate Input before running an analysis.
6. Open Solution Manager and run the desired model:
   - Model 1: PGA vs Distance
   - Model 2: Hazard Curve / Return Period
   - Model 3: Area-source PGA grid/map
   - Model 4: Return-period hazard map
7. Use Output Manager to review or export the available results.

TRIAL NOTE
This edition is intended for demonstration/evaluation. Some editing and user-defined functionality available in the Professional Edition is intentionally disabled.

Website: www.kamilkayabali.org/SeisHazard
